SSDS Communication Protocol

Version 1.0

## Description

There are two BLE characteristics provided by the ESP32, the Control characteristic and the Data characteristic:

|  |  |  |  |
| --- | --- | --- | --- |
| *Characteristic* | *UUID* | *Value Handle* | *Permissions* |
| Control | 0000**abc0**-0000-1000-8000-00805f9b34fb | 0x002a | R/W |
| Data | 0000**abc1**-0000-1000-8000-00805f9b34fb | 0x002d | R/W/N |

Commands from the app to the station are

## Protocols



